**Battery Care and Information**

**Before First Use**

When you receive your Eco-Glide PT

Charge the machine to 100% before first use.

The charger will show red while charging and switch to green when it’s done.

DO NOT leave your charger plugged in after the unit is charged.

Always remove the charger when you are finished charging.

•

**Conditioning**

**a new battery**

by using it until it is fully discharged or to 20% and then re-charge it fully. Doing this once a month will help to accurately calibrate your battery. Only do this if you are planning to ride the unit.

Always

**ensure the battery is recharged as soon as possible after it becomes fully discharged**

. A battery will be permanently damaged if left for an extended length of time in a fully discharged state.

**Remove the battery if storing for several months**

(the battery should be at approximately 50% charge or higher).

Do Not - Expose the battery to

**excessive heat or cold**

(i.e. outside the range of 0-110 degrees ambient).

A **battery** that provides 100 percent capacity at 80°F **will** typically deliver only 50 percent at **0**°F. **Put** simply, cold weather **will** decrease **the** lifespan of **your battery** because it **will** require charging more often.

•

Do Not -

**Store the battery in a fully charged state**

(store batteries with about 50%charge).

Keep your lithium batteries in a place that does not get colder than **32 degrees Fahrenheit** or warmer than 80 degrees Fahrenheit.

The battery can be remove from the machine with 6 Allen screws. DO not remove the battery from the battery enclosure.